Bid #151519 Septic Removal Q&A

* What are the specs for the new tanks? *2,000 Gallon minimum precast tanks with baffle for strength, baffle will likely need to be drilled at bottom for flow.*
* How much gravel under tanks? *6” minimum Limestone gravel base*
* How far apart are the tanks? *2ft minimum between tanks*
* What are the pump motor specs? *.5 hp 460v pump*
* Will they (vendor) need a licensed electrician for install? *provide licensed electrician for motor controller connections*
* Will they (vendor) need to include a warranty and or maintain system? If so, what is the timeframe? *1 year warranty only on items installed*