**FOOD COURT**

ITEM NO. 01 STORAGE SHELVING

1. Three (3) - Metro Max Q on casters 36 x 18 x 74, 4 shelves

# ITEM NO. 05 3-TIER MOBILE MICROWAVE CONVECTION OVEN W/ STAND

1. One (1) - TurboChef, consisting of one (1) Single Batch Oven and one (1) Double Batch Oven.
2. To include:
   1. Model HHS-9500-1 single oven.
   2. Model HHS-9500-814-DL double oven. 03 Stainless steel exterior finish.
3. Stainless steel interior.
4. Model HHD-8485 Stacking Kit.
5. Model NGC-1217-2 18" high Oven Cart.
6. Six (6) model 100018 PTFE cooking screen. 08 One (1) model NGC-1478 aluminum paddle. 09 One (1) bottle of oven cleaner.
7. One (1) bottle of oven guard.
8. Two (2) trigger sprayers.
9. Special Instructions:
   1. Mount ovens on stand per manufacturers recommendations. 02 Anchor ovens to stand.

# ITEM NO. 06 MICROWAVE OVEN

1. One (1) - Panasonic, model NE-1064F.
2. To Include:

01 Cord and plug.

1. Special instructions:
   1. Restrain excess cord length.
   2. Install on Item No. 04, Back-Up Table.

# ITEM NO. 07 PANINI GRILL

1. One (1) – Waring Model WDG250T

Grooved top and smooth bottom Panini Sandwich grill with timer

14 ½” x 11” cooking surface

120v 1800w.

# ITEM NO. 08 MOBILE UNDERCOUNTER REFRIGERATOR

1. One (1) - Continental Refrigerator, model D48N-U.
2. To Include:

01 Stainless steel finish top, sides and doors. 02 Stainless steel finish interior.

1. Aluminum back.
2. Hinge doors per drawings. 05 Cord and plug.

06 1-3/8" dia. swivel casters.

1. Special Instructions:

01 Install into base of Item No. 04, Back-Up Table.

# ITEM NO. 09 COFFEE MAKER

1. One (1) – Fetco Model CBS-51H-15 Handle operated coffee brewer

# ITEM NO. 10 GRAB-N-GO CASE

1. One (1) - Federal Industries, model ITRSS6034-B18, self-contained.
2. To Include:
   1. Horizontal top light.
   2. Three (3) stainless steel shelves with lights below. 03 Stainless steel deck.
3. Reflective end glass.
4. Reflective glass rear sliding door.
5. Rear condensing unit air intake and discharge. 07 Condensate evaporator assembly.

08 Adjustable leg levelers. 09 Cord and plug.

10 Plastic laminate exterior finish. Color selected, by Architect, from manufacture's standard colors.

1. Ancillary Equipment:
   1. Two (2) filler panel size and shape per detail. Construct of ½" MDFX board with black plastic laminate finish on all exposed surfaces. Mount on 14 ga. stainless steel, channel toe base per details.
2. Special instructions:
   1. Provide opening in base for electrical cord access to floor receptacle. Coordinate location of cut-out with receptacle.
   2. Restrain excess cord length.
   3. Extend electrical cord and plug to receptacle.

# ITEM NO. 15 BLENDER

1. Two (2) - Vitamix, model 062824.
2. To Include:

01 48 oz clear high-impact container. 02 Cord and plug.

* 1. One (1) additional Blender Container model 15978 for each unit.

1. Special Instructions:

01 Install on Item No. 13, Back-Up Table.

# ITEM NO. 16 CONDIMENT & LID DISPENSER

1. One (1) - Dispense-Rite, model WLO-1B.
2. To Include:
   1. Counter mount.
   2. Removable dividers.
3. Special Instructions:
   1. Install on Item No. 31, Beverage Counter.

# ITEM NO. 17 REFRIGERATED DISPLAY CASE

1. One (1) - Federal Industries, model SGR5048, self-contained.
2. To Include:

01 Tilt-out glass front. 02 Horizontal top light.

03 Three (3) white wire shelves with lights below. 04 Removable white deck.

05 Reflective end glass.

06 Reflective interior rear doors. 07 White interior finish.

08 Black exterior rear finish.

09 Condensate evaporator assembly.

1. Adjustable leg levelers.
2. Cord and plug.
3. Joining Kit.
4. Plastic laminate exterior finish. Color selected, by owner, from manufacture's standard colors.
5. Ancillary Equipment:

01 Filler panel size and shape per detail. Construct of ½" MDFX board with black plastic laminate finish on all exposed surfaces. Mount on 14 ga. stainless steel, channel toe base per details.

1. Special instructions:
   1. Provide opening in base for electrical cord access to floor receptacle. Coordinate location of cut-out with receptacle.
   2. Extend electrical cord and plug to receptacle. 03 Restrain excess cord length.

# ITEM NO. 18 AMBIENT DISPLAY CASE

1. One (1) - Federal Industries, model SGD5948.
2. To Include:

01 Tilt-out glass front. 02 Horizontal top light.

* 1. Three (3) white wire shelves with lights below. 04 Removable white deck.

05 Reflective end glass.

06 Reflective interior rear doors. 07 White interior finish.

08 Black exterior rear finish. 09 Adjustable leg levelers.

1. Cord and plug.
2. Plastic laminate exterior finish. Color selected, by owner, from manufacture's standard colors.
3. Ancillary Equipment:

01 Filler panel size and shape per detail. Construct of ½" MDFX board with black plastic laminate finish on all exposed surfaces. Mount on 14 ga. stainless steel, channel toe base per details.

1. Special instructions:
   1. Provide opening in base for electrical cord access to floor receptacle. Coordinate location of cut-out with receptacle.
   2. Extend electrical cord and plug to receptacle. 03 Restrain excess cord length.

ITEM NO. 23 ESPRESSO CAPPUCCINO MAKER

1. Two (2) - Scharer Coffee Atrs Plus

* Aesthetic design for high visibility concepts
* Capacity finesteam technology
* Up to 70-80 cappuccinos/lattes per hour (16oz)
* Dual bean hoppers with dedicated grinders
* Easy to operate and clean

Specifications:

* 208V, 30 Amperes
* NEMA L6-30R Receptacle
* 17“ (W) x 22“ (D) x 28“ (H)
* 6kW Steam Boiler

# ITEM NO. 24 MOBILE UNDERCOUNTER REFRIGERATOR

1. One (1) - Continental Refrigerator, model D48N-U.
2. To Include:

01 Stainless steel finish top, sides and doors. 02 Stainless steel finish interior.

1. Aluminum back.
2. Hinge door per drawings. 05 Cord and plug.

06 1-3/8" dia. swivel casters.

1. Special Instructions:

01 Install into base of Item No. 19, Serving Counter.

# ITEM NO. 26 MOBILE REFRIGERATED MAKE TABLE

1. One (1) - Continental Refrigerator, model PA60N-D.
2. To Include:

01 Stainless steel finish top, front and sides. 02 Stainless steel finish interior.

03 Stainless steel insulated, hinged, removable flat cover. 04 Full length 19" wide cutting board.

05 Stainless steel divider bars for 1/3th size pans. 06 Stainless steel roll-out drawers.

07 Compressor location per drawing. 08 Cord and plug.

09 5" dia. swivel casters with polyurethane tires.

1. Ancillary Equipment:
   1. Eight (8) Vollrath, model 90342, 4" deep, 1/3th size stainless steel pans.
   2. Seven (7) Vollrath model 90062, 6" deep, full size stainless steel pans.

# ITEM NO. 27 WALL SHELVING

1. One (1) lot - Eagle Group, "QuadTruss" model GWB with "EAGLEgard" epoxy finish. Two (2) tier ( upper & lower level) of wall mounted shelves.
2. Each level to consist of:

01 Two (2) QuadTruss single stationary wall mount brackets. 02 One (1) QuadTruss double stationary wall mount bracket. 03 Two (2) QuadTruss wire shelves.

1. Shelf size each level: 01 Two (2) 18" x 36".
2. Special instructions:

01 Assemble sections, as shown on drawings, into single shelf unit. 02 Provide anchoring material for wall mounting.

* 1. Set shelf height for each level as instructed by Owner.

# ITEM NO. 29 MOBILE UNDERCOUNTER REFRIGERATOR

1. One (1) - Continental Refrigerator, model D36N-U.
2. To Include:

01 Stainless steel finish top, sides and doors. 02 Stainless steel finish interior.

03 Aluminum back.

04 Hinge doors per drawings. 05 Cord and plug.

06 1-3/8" dia. swivel casters.

1. Special Instructions:

01 Install into base of Item No. 13, Back-Up Table.

# ITEM NO. 34 CONDIMENT & LID DISPENSER

1. One (1) - Dispense-Rite, model WLO-1B.
2. To Include:
   1. Counter mount.
   2. Removable dividers.
3. Special Instructions:
   1. Install on Item No. 31, Beverage Counter.

# COFFEE KIOSK

# ITEM NO. 44 UNDERCOUNTER REFRIGERATOR

1. One (1) - Continental Refrigerator, model UC24SN.
2. To Include:

01 Stainless steel finish top, sides and doors. 02 Stainless steel finish interior.

1. Aluminum back.
2. Hinge door per drawings. 05 Cord and plug.

06 1-3/8" dia. swivel casters.

1. Special Instructions:

01 Install into base of Item No. 41, Back-Up Counter. 02 Coordinate installation with Millwork Contractor.

03 Coordinate clearance below bottom edge of top with height of mobile equipment. Equipment to fit under top unobstructed.

# ITEM NO. 46 DUAL TEMP DISPLAY CASE

1. One (1) - Federal Industries, model SGR5042DZ, self-contained, non-refrigerated ambient section with refrigerated section.
2. To Include:
   1. 35" deep case.
   2. AMBIENT SECTION
      1. Tilt-out glass front.
      2. Horizontal top light.
      3. Two (2) white wire shelves with lights below.
      4. Removable white deck.
      5. Reflective end glass.
      6. Reflective interior rear doors.
      7. White interior finish.
   3. REFRIGERATED SECTION
      1. Tilt-out glass front.
      2. Horizontal top light.
      3. Two (2) white wire shelves with lights below.
      4. Removable white deck.
      5. Reflective end glass.
      6. Reflective interior rear doors.
      7. White interior finish. 04 Black exterior rear finish.
3. Condensate evaporator assembly. 06 Adjustable leg levelers.
4. Cord and plug.
5. Plastic laminate exterior finish. Color selected, by owner, from manufacture's standard colors.
6. Ancillary Equipment:
   1. Filler panel size and shape per detail. Construct of ½" MDFX board with black plastic laminate finish on all exposed surfaces. Mount on 14 ga. stainless steel, channel toe base per details.
7. Special instructions:
   1. Extend electrical cord and plug to receptacle.
   2. Provide opening in base for electrical cord access to floor receptacle. Coordinate location of cut-out with receptacle.
   3. Restrain excess cord length.

# ITEM NO. 47 COUNTERTOP PASS-THRU REFRIGERATOR

1. One (1) - True Food Service Equipment, model GDM-05PT-S-HC-TSL01.
2. To include:

01 Stainless steel exterior finish. 02 White epoxy interior finish.

03 Stainless steel interior floor. 04 Glass doors.

1. Two (2) epoxy coated shelves.
2. Door locks.
3. Cord and plug.
4. Special Instructions:

# ITEM NO. 55 FOOD SHIELD

1. One (1) lot - Versa-Gard, model VG24, vertical glass protector.
2. To Include:
   1. Mounting option C1 with flange at counter top.
   2. I" dia. solid 6061-T6 aluminum supports and mounting hardware. 03 Brushed aluminum with satin clear anodized finish.
3. Intermediate glass support as required.
4. 1/4" thick tempered glass front protector. Radius all corners.
5. Special Instructions:
   1. Submit shop drawing of food shield.
   2. Coordinate installation with Millwork Contractor.
   3. Secure food shield mounting bracket to underbracing of counter top. Mount food shield per manufactures recommendations.

# ITEM NO. 56 UNDERCOUNTER REFRIGERATOR

1. One (1) - Continental Refrigerator, model UC24SN.
2. To Include:

01 Stainless steel finish top, sides and doors. 02 Stainless steel finish interior.

03 Aluminum back.

04 Hinge door per drawings. 05 Cord and plug.

06 1-3/8" dia. swivel casters.

1. Special Instructions:

01 Install into base of Item No. 45, Serving Counter. 02 Coordinate installation with Millwork Contractor.

03 Coordinate clearance below bottom edge of top with height of mobile equipment. Equipment to fit under top unobstructed.

01 Install on Item No. 45, Serving Counter.