ROOF REPLACEMENT AT THE CHEROKEE NATION MARSHALL BUILDING
September 30th, 2026 
  
Clarification to the roof specification 
This addendum is hereby a part of those documents and contracts, the same as if bound therein and it shall supersede anything contained in the original bid manual with which it might conflict. 


- At Marshall Building: 
-For base bid system, KEE single-ply membrane shall be heat welded at all side laps and end laps. 
-At RTU’s marked for removal, curbs are to stay in place once unit is removed. Once units are removed, build up perimeter of curb with 2X to accommodate 8” flashing height. Install wood supports 16” o.c. fastened to perimeter curb. Install ¾” plywood mechanically fastened to top of curb. Install single-ply PVC membrane over top of plywood. Install 24 ga. galvanized metal cap with soldered corners and seams. Fasten metal cap through side of curb with appropriate fastener 12” o.c.  
-All antennas shall be removed from the roof and provided to the owner.
-Existing conductor heads and downspouts shall be salvaged. When replacing scupper inserts, ensure that scupper inserts are soldered completely and angled toward downspout for positive slope.  
-Electrical conduit located on East and South perimeter will not be abolished and shall be reinstalled and secured to interior face of new metal coping cap.
-At the designated units to be raised, install new curb adaptors along with new piping connection points. Units to be raised will be marked with a blue “X”. For base bid system, seal behind top of flashing membrane at curb flashings with water block sealant prior to installing counterflashing. For alternate system, 5-course top of flashing membrane at curb flashings with mastic and reinforcement fabric before installing termination bar and counterflashing. 
-At both open atriums, interior coping at North, East, and West atrium perimeters shall not receive new coping metal. Existing access ladder at Southeast atrium shall stay in place.
-Gas lines designated for removal are marked with spray paint. Mechanical contractor is to remove and cap or plug gas line at the furthest connection.
-Refer to roof overview below with areas marked to receive new expansion joints. For base bid system, both expansion joints shall follow KEE “low profile” expansion joint detail drawing and installation instructions. For alternate system, both expansion joints shall be Johns Manville EJ-6 expansion joints utilizing 2 X 6 wood blocking to match insulation thickness secured 3” o.c.
-At condenser marked for removal at Southwest perimeter, install new 6” X 6” pitch pan with new square hood. 
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New Expansion Joints
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Note:

Dimensions to be field verified by contractor.




