ROOF REPLACEMENT AT THE CHEROKEE NATION MARSHALL BUILDING
October 7th, 2026 
  
Clarification to the roof specification #2  
This addendum is hereby a part of those documents and contracts, the same as if bound therein and it shall supersede anything contained in the original bid manual with which it might conflict. 


- At Marshall Building: 
-For alternate system, flashing backer sheet and flashing membrane shall both be set in flashing adhesive prior to heat welding side laps and cant/membrane transition of flashing backer sheet and flashing membrane.
-At curbs to be covered with metal cap, provide slope in metal cap to ensure positive drainage toward scuppers. 
-Include as an add-alternate for both base bid and alternate bid: Contractor shall provide and install new ¾” condensation lines and new 2” main lines that condensation lines will tie into. No more than five (5) condensation lines are to tie into a single 2” main line. New main lines are to run the full length to the nearest scupper in which the downspout drains underground. Main lines shall not run to a scupper where the connecting downspout drains onto the pavement. New condensation and main line piping shall be Type L Copper. Traps shall be provided by the owner and installed by the owner. 
-Owner shall install three (3) roof hydrants once existing roof is removed down to the steel decking. Owner will be responsible for cutting three (3) holes into steel decking and installing roof hydrants. Contractor shall install pitch pans around each roof hydrant. Set hydrant in non-shrink grout inside pitch pan. Fill top with pourable sealer. Cap pitch pan with new hood. Install band on top of hood and seal band with sealant as specified. 
-At curb and wall transitions, omit new horizontal wood blocking referenced in detail drawings. See revised detail drawings below for reference.
[image: ]


[image: ]



[image: ]
image1.tif
SECTION A-A

TURN ENDS DOWN
45'ANGLE

SEALANT BETWEEN
METAL SECTIONS

NEOPRENE GASKETED
FASTENER 24" O.C.

CONTINUOUS CLEAT
FASTENED 16" O.C.

ATTACH NAILER TO
WALL

FLASHING MEMBRANE
INSTALLED OVER
NAILER

BASE FLASHING

TWO-PLY STRIPPING

MULTI-PLY MODIFIED
BITUMEN ROOFING

CANT STRIP

SPECIFIED INSULATION

ROOF DECK

SHEET TITLE: SCALE.

- NTS
v , TREMCO METAL COPING CAP DRAWING No.

Roofing & Building Maintenance DWG NO. 03

B





image2.tif
NON-LIFTABLE

APPROVED SEALANT
BEHIND TOP OF FLASHING

MECHANICAL UNIT
|
i ©

GALVANIZED ANNULAR
RING SHANK NAILS
@"0.C)

OOF TOP UNIT

OR SKYLIGHT

METAL COUNTERFLASHING, FASTEN W/
EPDM WASHERED FASTENERS (12" 0.C.)

TREMPLY KEE FLASHING (FULLY ADHERED)

/——EPDM WASHERED FASTENER
AS REQUIRED

8" MIN. ’
L L]

< L}
E:
‘°°

2%
% 5o
9 4

‘WOOD CURB CONSTRUCTION/Z

INSULATION ATTACHE

TREMPLY KEE MEMBRANE FLASHING
ADHERED IN TREMPLY KEE LV BONDING
ADHESIVE

PREMOLDED CORNER
HOT AIR WELD

TREMPY KEE
MEMBRANE

SPECIFICATION REQUIREMENTS

APPROVED ALUMINUM TERMINATION/
RESTRAINT BAR FASTENED

WITH APPROVED FASTENERS
(8"0C)

SHEET TITLE:

SCALE:

vp» TREMCO

Roofing & Building Maintenance

TYPICAL WOOD OR SKYLIGHT CURB
FLASHING (BLOCKING ALTERNATE)
T-BAR RESTRAINT

NTS

DRAWING No,
DWG NO. 124

B





image3.tif
I

TREMPLY KEE MEMBRANE FLASHING
TREMPLY KEE LV BONDING ADHESIVE

-APPROVED 1/8" X 1" ALUMINUM BAR
ATTACHED (8"0.C.)

HOT AR WELD

TREMPLY KEE MEMBRANE

—INSULATION ATTACHED PER
SPECIFICATION REQUIREMENTS

:
¢

ETTrTrrereTY)

—
IR
SIRELIRRIK
RRIRELIKERS
$IRIBRIKKRS
RRRRRRLRRRRKRS

N

7

TREMPLY KEE MEMBRANE FLASHING

TREMPLY KEE LV BONDING ADHESIVE

WOOD BLOCKING
ATTACHED @ 250 LBF/FT

HOT AR WELD
TREMPLY KEE MEMBRANE

INSULATION ATTACHED PER
SPECIFICATION REQUIREMENTS

-

Z

vp» TREMCO

Roofing & Building Maintenance

SHEET TITLE: SCALE:

WALL FLASHING ALTERNATE NTS

DRAWING No,
DWG NO. 131

"BASE" SECUREMENT

B





