RFP #164709 Questions and Answers-
Scope of project notes:
1. Pendant “D” light fixtures, same spec, but color will change to a Satin Nickel finish.
2. Remove Sound masking from scope of work, will be by CNB I.T..
3. All door heights to be 7’-0”, unless noted otherwise.
4. All ceiling grid and tiles to be new. Ceiling tile USG 2220.
5. All lever door hardware is to match existing on this floor, black finish is no longer being used.

Q: Can you clarify what we are to bid for ceiling grid and tile? Scope of work says “Contractor to provide allowance for repair, replacement and painting of ceiling grid”. In Finish Plan Legend on sheet A4.0 it says “For alternate price of new ceiling tiles, match tile on floors 14/15”. On sheet A2.0 it says “new acoustical ceiling tile 2x2 set in existing grid. Paint all exposed ceiling gid and match ceiling tiles on 16th floor. This is very confusing. Can you tell us exactly what base bid is and what alternate is and scope of what we are to include in both?

A: Revised. No alternates in scope of work. All ceiling tile and ceiling grid will be new. Ceiling tile is USG2220.

Q: Is the ceiling the only alternate? Any allowances on the project we need to include?
A: No


Q: Is there a bid form or any other bid documents we need to submit?
A: You will submit your bid following the instructions on Cherokeebids.org website under bid #164709.

Q: Is performance and payment bond needed on this project? Bid bond?
A: No

Q: Is there a door, frame, and hardware schedule? Sheet A1.1 lists doors in legend, but vague on what is required and says to match existing. With fail safe being incorporated on some doors and the complexity and variations of doors and hardware on the market, bidding this without more information will be very tough and not apples to apples between suppliers.
A: There is no door, frame and hardware schedule. All doors are to match existing unless noted otherwise. They are 3’X7’ doors, all hardware to match existing unless noted otherwise.

Q: Is there any window or storefront elevations or schedule showing type and sizing?
A: No, refer to floor plan and floor plan key legend. Refer to one of the other Cherokee Federal floors, can look at 16th floor WCTII.

Q: Do we install blinds on ALL windows?
A: No, they will be done by the Owner


Q: Finish plan note 9 on sheet A4.0 says to replace all existing doors to match existing with black lever hardware. With no door schedule, it is tough to know exactly what doors to replace. Can architect mark these doors on plan and specify exact hardware?
A: All door hardware is to match existing, no longer using black finish.

Q: Per Drawing A3.0, Note 12, All Electrical & Data not indicated with “N” is existing and is to remain. Per Scope of Work, Bullet Point #7. Existing cable is to be removed. Please verify which is correct.
A: any existing cable not used, so not shown with “E” is to be removed.

Q: If existing cable is to remain, do the Jacks, Faceplates, and Patch Panels need to be changed to Panduit?
A: TBD

Q: Per Drawing A3.0, Please verify all data symbols with “N” are a single cable or dual cables.
A: TBD

Q: A4.0 Finish Plan Legend says: LVT: Cabinet/Millwork Fronts LVT1 Shaw Rethink Hybrid 33100. I assume this is simply mislabeled. Please advise.
A: This is text error, LVT1 is Shaw, rethink and PL1 is Wilsonart.

Q: Floor plan shows blank boxes in many offices, Break and Conference. Please confirm these are not millwork items.
A: These are building columns.
 
Q: Existing Mens & Womens Restrooms. Sheet A1.1. Floor Plan Key Note #5: Finish Upgrades.  What are the expectations of the millwork provider in this scenario? Refinishing wood cabinets? Relaminating laminate cabinets?
A: Not applicable, there are no cabinets in the restrooms. Existing millwork under vanities to be removed. Refer to sheet A5.1, elevation D and F for vanity elevation, to be similar. Exposed plumbing to be wrapped per ICC A117.1-2009 requirements.

Q: C3 carpet shown on finish plan legend but not shown on plans. Please confirm where this carpet type is located.
A: C3 not used.

Q: CG1 corner guards shown on finish plan legend but not shown on plans. Please confirm location of corner guards.
A: CG1 not used.


Q: Could you find out the deck heights and the ceiling tile number we need to match per this note:
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A: ceiling tile is USG 2220

Q: Please confirm bonding is not required for this project.
A: Bond is NOT required


Q: Please confirm builders’ risk is not required for this project.
A: Yes, it is required


Q: Please confirm this project is NOT tax exempt.
A: It is NOT tax exempt


Q: Is there any specification information on 2x2 or 2x4 lay-in tiles? Will they be owner-furnished?
A: They are not owner furnished and ceiling tiles are USG2220.

Q: What is species type of wood doors and what are height and width requirements?
A: Match existing species and stain. Doors are 3’X7’, unless noted otherwise.

Q: The 45-minute door cannot have a full view glass. Will this require a smaller size glass? 
A: Full view glass is allowed and was done on the 16th floor of WCTII, Cherokee project in 2024. Refer to door detail, sheet A5.0, elevation “A”, door height will be 8’-0” and not 9’-0” as listed.

Q: Verifying if job is tax exempt and Davis Bacon wage scale?
A: No and No

Q: Will there be a designated parking area?
A: We can make a few parking spots under the building available but not for the subs.  They can park at the City Parking garage 100 W. Boulder or in the lot directly north of Tower II at 2nd & Boulder.

Q: Will a window be removed for stocking the project or, will we utilize the existing elevators?
A: Use Freight Elevator.


Q: The 16th floor has a mixed variety of ceiling tile however, the predominant ceiling tile appeared to be USG #2220. Would this be the tile standard?
A: Spec is USG 2220.

Q: Finish plan legend on sheet A4.0 shows "match tile on floor14/15." Upon site visit, the 15th floor ceiling tile appears to be the same as the 16th floor. "USG 2220". The 14th floor shows predominant ceiling tile to be Armstrong tile #934A. This ceiling tile would be a residential version of the Armstrong tile #770. Would it be acceptable to figure the identical commercial tile in lieu of the residential? 
A: Spec is USG 2220.

Q: Can the existing lights be used for this project?
A: No, same lights as 17

Q: If yes, how many of each type are there?
A: N/A

Q: What is the manufacturer and model number of ALL building standard light fixtures?
A: light fixture specification is: Cooper Lighting, Metalux, 24CGTS-L3C3

Q: Can standard stainless device plates be used?
A: No, match existing.

Q: What is the building standard for floor boxes?
A: Hubbell 4” box or similar.

Q: Is the 3rd floor lay-in ceiling so poke-thru type floor boxes can be added/accessed?
A: Yes.

Q: What is the “approved” scanning method for core drills?
A: No specific method. Once core location is determined, contact building management before proceeding for approval.

Q: Note #10 on A3.0 refers us to sheet “A1.2”. That is not in the bid set documents. Please clarify.
A: Sheet A1.2 is the enlarged plan and plumbing schedule and should be included in the bid documents.

Q: New frames are called out as aluminum to match existing. I’m verifying that you have quotes coming from aluminum guys and are not expecting those from us? 
A: Unsure how to answer this question. Coordinate with your door framer.

Q: According to the floor plan legend, there are several doors to remain as is. Please verify that we do not need to include these in our quote.
A: Yes, several doors are to remain as is, do not include in quote.

Q: Pertaining to question 2, please verify that we do not need to include new hardware in openings designated to remain as is.
A: No new hardware is needed if doors are to remain, if hardware is missing, add new.

Q: Are there any special keying requirements to consider on any of the new hardware?
A: none needed.

Q: On the floor plan legend, 400 elevator lobby doors are wood in an aluminum frame, but the A elevation shows them as TPG designer glass doors. Please verify
A: Error on H type door in floor plan, sheet A1.1. The elevation, “A” sheet A5.0 is correct.
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