PACE Ornamental Fence Specifications
Manufactured in the USA
Equal to or better than Ameristar Montage Plus, (Classic style three rail steel ornamental fence, Black in color). 
Follow all the Manufacturers’ installation instructions.
Fencing shall have a minimum of a 20-year manufacture  warranty.
Pickets: .75"sq x 18ga
Rails: 1.4375" x 1.5" x 14ga
Posts: 2.5"sq x 16ga
Heights: 4'
IBC Compliant Configuration:
· 3 rails
· 2.5"sq. x 14 ga. min posts
· All brackets (flat mount and swivel must be thru-bolted) 
· For plated posts: 8" x 8" min plates with gussets
3 Rail Panels
·  4' height
· Standard bottom rail 
· 4" standard picket airspace 

Pricing shall include all materials and installation costs for a 100% complete project.




