RFP #164809 Questions and Answers-

Q: Lighting protection on both towers is not re-usable; coating most likely made the copper lose its conductive properties needed to do the job it is designed for. A guaranteed adhesion is needed. 
A: If existing LPS is unsuitable for re-installation, pricing a new system would be acceptable.

Q: Electrical Conduits ran on bottom side of deck will most likely be punctured and damaged during the Roof overlay prosses. Would there be an appointed electrician to contact for this project?
A: All electrical must be mapped and fasteners placed without damaging conduits where possible. Any damage to electrical system or conduits will be the responsibility of the roofing contractor to repair or replace.

Q: Ladder being extended or removed and replaced? (On Tower II)
If the ladder is being removed and replaced, the Wall panel system will have to be removed. The wall panel system is starting to show signs of failer, face screws and caulking to hold together a buckling panel system with some open areas on both buildings allowing water into the envelope system. Mineral wool and Z furring were seen behind wall panel coming off of wall on Tower II. 
Would temporary repairs or remedies be quoted as an ALT?

A: Any repairs or remedies related to removal of any part of the roofing or wall system would be required as part of roofing contractor's alternate bid regarding the roof ladder.

