Scope of Work: 
Studio A MDF to Studio A IDF Connection
A 48-strand OS2 single-mode fiber will be installed between Studio A Main Distribution Frame (MDF) and Studio A Intermediate Distribution Frame (IDF), which serves the studio equipment. Panduit enclosures and bulkheads are preferred for this installation, with LC/LC termination specified. Of the 48 strands, 24 will be terminated for immediate use, while the remaining strands will be reserved as spares to accommodate future expansion needs. 
Studio B IDF to Studio A IDF Connection
Another 48-strand OS2 single-mode fiber will be run between Studio B IDF and Studio A IDF (studio equipment IDF), utilizing Panduit enclosures and bulkheads as the preferred hardware, and LC/LC termination. As with the previous connection, 24 strands will be terminated, leaving the rest available as spares for potential expansion. 
Conduit and Routing Considerations
The route between Studio A MDF and Studio A IDF will be entirely indoors. The existing conduit between Studio A MDF and Studio B IDF must be inspected to determine if it is wide enough to allow another fiber cable to be pulled through. Depending on the results of this inspection and the specifications of the previous vendor's installation, it may be necessary to bury additional conduit to support the new fiber run. 



Mandatory prebid Monday, August 8, 2026 2pm-3pm

Location: Cherokee Film Studio
                     16990 OK-20
      Owasso, OK 74055

