Scope Of Work-Split Rail Fence

124 E. Choctaw St. Tahlequah, OK 74464

1. Contractor should remove all existing fence and poles from the property and replace with new split rail fencing and poles.
2. Can re-use existing holes for the new poles as it coordinates with the property layout.
3. Contractor is responsible for building new gates and furnishing all gate hardware to match the iron hardware style. All hardware should be black in color.
4. Concrete will be use for the poles unless otherwise noted that a better solution could be used.
5. Contractor is responsible for disposing of all the old fence, clean-up, and any damage other than natural work-related causes to the grounds.
6. **Owner will provide the posts**, measurements for holes are 4-1/2" high and 1-3/4" wide
7. A possible timeframe of completion will need to be expressed.
8. If deemed necessary, work performed may need to be after hours or on closed days. This will be determined by Project Management.

Thank you

CPM Facilities,