New Cattle Trailer Specifications

Ranch Hand Tarp Top

Gooseneck

Rubber Floor

LENGTH 24' 0"

WIDTH 6' 8"

HEIGHT: 6' 6"

Twin Axle 7,000 lbs or more

Electric brake

36" side escape door

full swing rear gate with slider

16 ga. formed slats

2 center gates

tube slat drop wall for airflow

LED load light on rear

Spare tire