RFP #164912 Questions and Answers-

Q: Will CN accept an alternate roofing system that meets all criteria of specified roofing system with the exception of the ASTM D6754-15 Tremco Product? 
A: Yes. However, all RFP requirements must be met; this includes all manufacturer delineated responsibilities as listed in Section 1.03 and Section 1.10.


Q: Will CN accept a 10yr maintenance warranty program from the contractor?
A: No.


Q: Will a bid bond and performance bond be required on this project?
A: A payment and performance bond will be required. A bid bond is not required.


Q: Specification Section II, paragraph 8.01, mentions “Provisions for Liquidated Damages, if any, will be specified in the Statement of Work”, but nothing was listed.  Will there be liquidated damages and, if so, what is the daily dollar amount?
A: No liquidated damages.


Q: Specification Section V, where it talks about “Bonds” (Bid Bonds, Performance & Payment Bonds, Maintenance Bond) it just says they will be required “if required per the Statement of Work”.  However Section III “Statement of Work” does not mention anything about any of these bonds.  Will any of these bonds be required?

A: Bid Bond-not required.
Performance and Payment Bond-required.
Maintenance Bond-not required.

Q: There is currently electrical conduit mounted to the top of the concrete parapet wall along the E. end of the building and along a portion of the S. side of the building.  It was discussed at the pre-bid meeting that CN would investigate whether or not the wiring in this conduit is still live or dead, and whether the roofing contractor will be permanently removing this conduit if the wiring is dead, or having an electrician relocate the conduit and wiring if it is still live.  Please clarify.
A: Electrical conduit located on East and South perimeter will not be abolished and shall be reinstalled and secured to interior face of new metal coping cap.

Q: Would Cherokee Nation Builders consider in lieu of raising curbs and capping all of the skylights and 10 RTU's that will be removed to allow us to demo out the curbs and inlay metal deck?  Then we would install the specified roof system over that.  This will allow for a better finished product with 37 less roof penetrations that will prevent the opportunity for potential issues in the future.
A: No. Infilling the curbs require a structural consideration; not just a decking insert. Therefore, the Owner has felt it easier to cap and preserve the curb for possible future use.




