EXHIBIT A
	UNIT
	UNIT
	PRICE

	Landscape maintenance to include mowing, fertilization/herbicide, shrub bed services and Irrigation services
	Month

	

	Irrigation repair
	hourly
	

	Seeding grass
	sq. ft/hourly
	

	Sod
	sq.ft./hourly
	

	Skid steer w/operator
	hourly
	

	Mulch installed 
	cu.ft./hourly
	

	Seasonal Color standard flat
	flat
	

	Seasonal Color Premium flat
	flat
	

	Labor to install seasonal
	hourly
	

	Spraying weeds in cracks
	hourly
	

	Brush Hog w/ operator
	hourly
	

	Tree trimming
	hourly
	

	Shrub trimming
	hourly
	

	Over seeding (including labor)
	hourly
	

	Planting trees up to 3"
	hourly
	

	Aeration hourly rate
	hourly
	

	Pre-Emergent 
	Application
	

	Post-Emergent
	Application
	


Generally, Contractor shall provide all labor, materials, equipment, tools and services required to provide 
full, professional lawn and landscaping maintenance and installation at Company’s Property (the “Work”),
Specifically, the Work shall include the following:
1. Base Services. Contractor shall perform the following Work on the Property on a weekly basis at 
the minimum, and more frequently as required by weather and growing conditions:
A. Turf Maintenance:
• Mowing, edging, blowing, and trimming of all turf areas. 
• Mowing height to be based on the season and what is horticulturally correct for the turf 
variety.  Weed eaters are acceptable for edging purposes.
• Mowing frequency shall be as required to maintain a lawn in the manner acceptable to 
Company’s Representative or designee (max height of 3”).
• Never scalp the lawn or remove more than 1/3 of the existing top growth in one mowing. 
During excessive periods of growth or after extended periods of rainfall, the turf is to be 
lowered in the appropriate manner possibly requiring multiple cuts.
• Any unsightly or visible clippings which remain on the turf are to be promptly removed. Mowers are to be equipped with Vacuum attachments to remove all grass clippings, pine needles and leaves as well.  Push mowers are to be used on the islands, and they must be equipped with bags to catch the grass clippings.
B. Shrub, Tree and Plant Maintenance:
• All suckers shall be continuously removed. Pruning for general cleanup of trees and
shrubs are recommended in the fall/winter season. All pruning cuts are to be made flush 
(“stubbing” will not be allowed).
• Periodically prune trees as needed to protect pedestrians or vehicular traffic (trees in 
pedestrian areas to be pruned with the canopy at 7’ or higher).
• All major pruning shall be done with the expressed authorization of Company’s 
Representative or designee and may require Company Security assistance to reduce 
potential safety risk.
• Remove all dead branches and diseased foliage immediately.
• Remove insect or disease infected plant materials.
• All trimming and pruning shall be performed to acceptable standards, with the correct 
equipment. Care must be taken not to use “weed eater” type machinery against the trees 
(Company, in its sole discretion, may require Contractor to replace trees damaged by weed 
eaters).
C. Turf and Bed Applications:
• Contractor shall notify Company’s Representative before commencing any chemical 
application program and all chemicals used on the Property must be approved by 
Company’s Representative and must conform to state or federal requirements.
• Material Safety Data Sheets for all chemicals used by Contractor on the Property shall be 
provided to Company’s Representative.
• Contractor shall strictly adhere to all OSHA or other regulatory agency safety laws, 
chemical manufacturer’s directions, and applicable Company policies and procedures in 
the use, storage and disposal of chemicals at the Property.
• Contractor is permitted to use such pesticides and chemicals as found 
necessary/advantageous. Chemicals shall be applied only by a properly licensed and 
approved pesticide applicator. Contractor shall provide Company with a current copy of 
the Oklahoma Agricultural Food and Forestry Division license that identifies the vendor as 
a certified applicator for the 3A Certified Applicator Category (Turf and Ornamental 
Outdoor).
• Contractor assumes all liability for damage and/or injury for use, storage and disposal of 
all chemical products or equipment.
• Contractor shall take all precautions necessary to eliminate chemical misuse, personal 
property damage, and/or damage to wildlife.
• Contractor shall notify the Company’s Representative in the event of any unusual circumstances regarding plant deterioration, wildlife death (mammal, fowl or fish) or other abnormal occurrences.
• All turf, beds and flowering shrubs shall be fed as needed (a minimum of two times and a 
maximum of three times per season) with a compatible fertilizer.
• All turf shall be treated with a Spring pre-emergent and a Fall pre-emergent weed control.
• Turf and beds shall be spot treated for weeds as needed.
• Herbicide spray shall be used to prevent growth in paved areas or areas where vegetated 
growth is not permitted.
D. All grass clippings, branches, cans, paper and other litter are to be removed from the landscape 
during the performance of the Work.
E. Irrigation – Irrigation system controls are to be properly maintained and operated. Appropriate 
timeframe for irrigation operation is from 2:00am to 8:00am in high traffic areas. Secondary 
areas can be operated outside of this timeframe with the permission of the Company’s
Representative
2. Additional Services. Additional Services shall include, but not be limited to, the following:
• Irrigation Repair - Repair of existing and installation of new irrigation systems (24-hour 
on call irrigation repair).
• Sod - Repair of existing and/or installation of new sod as requested by Company.
• Mulch – Mulch shall be placed annually in beds at a minimum of 2” in depth and as 
requested by Company.
• Seasonal Color – Contractor shall, upon Company’s request, procure standard and 
premium flats of seasonal colors and install the seasonal colors as directed by Company. 
Company shall reimburse Contractor for Contractor’s actual cost of the flats procured for 
installation on Company’s Property.
• Tree Planting – Contractor shall, upon Company’s request and direction, plant trees up to 
three inches (3”) in diameter.
• Tree Removal – Contractor shall, upon Company’s request and direction, remove trees 
from Company’s Property.
• Aeration – Contractor shall, upon Company’s request, aerate any areas as directed by 
Company.
• Design and Installation Services – Contractor shall, upon Company’s request and direction, 
design and install new landscaping on Property. Design services shall be performed by a 
certified landscape architect. Design and installation shall be performed within 24 hours of 
Company’s request.
• Other Callout Services – Company may request the lawn and landscaping services of 
Contractor for projects not covered by the Base Services or the listed Additional Services. 
Contractor shall provide Company with a cost estimate to perform the Callout Services. 
Contractor shall not incur any costs or begin performing any Callout Services without 
express authorization from Company or Company’s Representative.

All rates commence upon Contractor’s arrival at Company’s Location. Contractor’s travel time shall not be invoiced. Contractor’s rates are inclusive of all applicable costs for the provision of the Work including, but not limited to, expenses, permit costs and fees, including, without limitation, TERO fees, which fees shall be paid directly to the TERO office by Contractor, and other registration and/or licensing fees and rental expenses.

