Procurement 164729  Q & A 07.08.2026

Q:   Can you confirm whether the scope includes the removal and cleaning of the actual fill media, or if it is limited to the exterior components such as the louvers?


A:  Interior cooling tower fill media stays in place and cleaned in place. Exterior drift eliminator panels should be removed for cleaning (These are usually soaked in a solution)

